IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "2018_01"
Time stamp: "2020-09-25T18:16:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.1.0 - Alternativ-UI 20.2.1.0"
Application: "Autodesk Revit 2020 (DEU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (DEU)"

People and organizations
  Person "clevef6g" of Organization (no name given)
  Owner history of Person "clevef6g" of Organization (no name given) | application "Autodesk Revit 2020 (DEU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (DEU)" | change NOCHANGE | created 1601045430 (2020-09-25T14:50:30Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Ebene -1" | long name "Ebene -1" | object type "Ebene:Ebene" | elevation -0.3
        contains 4 elements
          1 x IFCSLAB | type IFCSLABTYPE "STB 1500 x 1500 x 500" | object type "Streifenfundament:STB 1500 x 1500 x 500" | FLOOR | names: "Streifenfundament:STB 1500 x 1500 x 500:2444317" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Pset_BIM
          1 x IFCSLAB | type IFCSLABTYPE "STB 1500 x 1500 x 500" | object type "Streifenfundament:STB 1500 x 1500 x 500" | FLOOR | names: "Streifenfundament:STB 1500 x 1500 x 500:2444339" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Pset_BIM
          1 x IFCSLAB | type IFCSLABTYPE "STB 1500 x 1500 x 500" | object type "Streifenfundament:STB 1500 x 1500 x 500" | FLOOR | names: "Streifenfundament:STB 1500 x 1500 x 500:2444358" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Pset_BIM
          1 x IFCSLAB | type IFCSLABTYPE "STB 1500 x 1500 x 500" | object type "Streifenfundament:STB 1500 x 1500 x 500" | FLOOR | names: "Streifenfundament:STB 1500 x 1500 x 500:2446261" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Pset_BIM
      IFCBUILDINGSTOREY "Ebene 0" | long name "Ebene 0" | object type "Ebene:Ebene" | elevation 0.
        contains 4 elements
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte:STB 300" | object type "Bodenplatte:STB 300" | BASESLAB | names: "Bodenplatte:STB 300:2444714" | material: layers "Bodenplatte:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Pset_BIM
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basiswand:LB 250" | object type "Basiswand:LB 250" | names: "Basiswand:LB 250:2445017", "Basiswand:LB 250:2445149", "Basiswand:LB 250:2445235" | material: layers "Basiswand:LB 250" ("Mauerwerk - ohne Dämmeigenschaften" 0.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | object type "Ebene:Ebene" | elevation 3.
        contains 1 element
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 300" | object type "Geschossdecke:STB 300" | FLOOR | names: "Geschossdecke:STB 300:2445749" | material: layers "Geschossdecke:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Types
  IFCSLABTYPE "STB 1500 x 1500 x 500" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "STB 1500 x 1500 x 500" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "STB 1500 x 1500 x 500" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "STB 1500 x 1500 x 500" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Bodenplatte:STB 300" | BASESLAB | 1 occurrence | material: layers "Bodenplatte:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basiswand:LB 250" | STANDARD | 3 occurrences | material: layers "Basiswand:LB 250" ("Mauerwerk - ohne Dämmeigenschaften" 0.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Geschossdecke:STB 300" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Property sets
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "STB 1500 x 1500 x 500" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "LB 250" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "STB 300" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "STB 1500 x 1500 x 500" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "STB 300" (IFCLABEL)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 1500 x 1500 x 500" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 300" (IFCIDENTIFIER)
    ThermalTransmittance = 3.48666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STB 1500 x 1500 x 500" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STB 300" (IFCIDENTIFIER)
    ThermalTransmittance = 3.48666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BIM | properties | on 2 objects (2 IFCSLAB)
    Familie und Typ = "Streifenfundament: STB 1500 x 1500 x 500" (IFCLABEL)
    TaskID = 6. (IFCCOUNTMEASURE)
  Pset_BIM | properties | on 2 objects (2 IFCSLAB)
    Familie und Typ = "Streifenfundament: STB 1500 x 1500 x 500" (IFCLABEL)
    TaskID = 11. (IFCCOUNTMEASURE)
  Pset_BIM | properties | on 1 object (1 IFCSLAB)
    Familie und Typ = "Bodenplatte: STB 300" (IFCLABEL)
    TaskID = 12. (IFCCOUNTMEASURE)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "LB 250" (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "LB 250" (IFCIDENTIFIER)
    ThermalTransmittance = 5.188 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "LB 250" (IFCIDENTIFIER)
    ThermalTransmittance = 5.188 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene -1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene 0" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene -1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene 0" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ebene 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "Projektadresse", "Platzl 9", "80331", "München", "Deutschland"